

**SQair**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – Belgium

Tel. +32 (0)56 62 71 11, fax. +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

****

dESCRIPTION

* Adjustable valve available in 4 versions
  + Extraction valve:
    - Basic: synthetic front plate RAL 9010 (coloured plastic)
    - Deluxe: Aluminium front plate (lacquered RAL 9010)
  + Pulse valve:
    - Basic: synthetic front plate RAL 9010 (coloured plastic)
    - Deluxe: Aluminium front plate (lacquered RAL 9010)
* Construction: grid base + front plate
* Protrudes only 24mm from the ceiling of wall.
  + The wider front plate conceals the ventilation openings.
* Direct connection onto the air ducts
  + Ø125mm
  + Integrated rubber gasket: airtight connection
* Front plate:
  + Basic: Snaps on the grid base
  + Deluxe: Attached with magnets to the grid base
  + Easily disassembled for cleaning
  + Thanks to the locknut the settings remain during cleaning
* The Pulse valve has 2 deflectors
  + 2 of the 4 ventilation openings can be closed using the deflectors.
    - For example: If the valve is installed close to a wall, this side can be closed to prevent the accumulation of dust.
* The pulse valve is provided with acoustic material
  + Prevents whistling noise at the valve

**Product features**

|  |  |  |
| --- | --- | --- |
|  | **BASIC** | **DELUXE** |
| Front plate | ASA | Aluminium |
| Measurements front plate | 170 x 170mm | 180 x 180mm |
| Measurements grid base | 150 x 150mm | 150 x 150mm |
| Colour | RAL 9010 | RAL 9010 |
| Attachment | Snap-on | Magnets |
| Paintable | - | Yes |
| Deflectors | - | 2 |
| Measurements deflector | 92 x 20mm | 92 x 20mm |