**Invisivent® AIR Light**

Renson Ventilation, IZ 2 Vijverdam, Maalbeekstraat 10, 8790 Waregem – Belgium

Tel. +32 (0)56 62 71 11, fax +32 (0)56 60 28 51, [info@renson.be](mailto:info@renson.be) www.renson.eu

product features (text marked in red can be deleted at your discretion)

* Type: Thermally broken, noise-reducing, self-regulating valve ventilation for installation on the window
* Acoustic comfort:
  + Equipped as standard with acoustic damping material   
    (PEPP – Porous Expanded Polypropylene)
  + Integrated acoustic material: no additional acoustic module to the inside
* Self-regulating valve (P3):
  + Self-regulating effect at pressure differences as of 2 Pa
  + Automatically responds to pressure differences/wind strength and cannot be influenced by the user
  + Ensures constant airflow and reduces energy losses
* Adjustable aluminium inner valve directs the airflow upwards: Coandă effect
* Non-punched, controllable inner valve with gripping edge: 5 positions
* Condensation-free, due to the thermally insulating profile on the inner valve
* Insect-proof: invisible, perforated inner profile (3.9 x 9.8 mm)
* Easy cleaning: Removable inner profile
* Controls: manual, cord, rod
* Finish:
  + Anodised (F1) / powder-coated in the same RAL colour as the window profiles / bicolour
  + Colour of endcaps = colour of window profile (colour differences are possible)
* Construction height: 65 mm / visible outside opening: 33 mm
* Recessed installation on the window profile (0 mm glass reduction):
  + Suitable for window profile thicknesses of 50 to 202 mm (and thicker on request)
  + Completely recessed installation both indoors and outdoors (completely invisible)
  + Optional designer outer cover available
* Perfect airtight connection to the window profile due to coextruded, flexible sealing over the entire length of the window ventilation, including the endcaps.
* Installation:
  + Directly anchor the window ventilation to the window with screws
    - Screw zone provided in the PVC body
    - Additional screw zone through the aluminium outer profile makes it possible to anchor the product at any time without damaging the thermal bridge of the window profile
    - Quick and easy installation due to the monobloc principle
  + Guaranteed stability of window and louvre due to monobloc principle + additional reinforcement with screws in body (every 280 mm)
  + Integrated Euronut dowel slot for good anchoring to the wall
* Flexible and aesthetic interior finishing:
  + Airtight wet plastering: easy to do due to removable vertical rib, which allows a standard plaster profile (commercially available) to be used.
  + By removing the vertical rib, a recess is created in which an MDF board, plasterboard, or PVC panel can be placed.
  + A buffer area prevents plastering of the inner valve
* Optionally available with Pollux filter: for rooms with high particulate and pollen levels

APPLICATION

* Can be combined with Invisivent COMFORT in the same project due to the identical look & feel
* Dimensioned at 2 Pa: can be used in every project as standard

performance level

* **U value**: 2.0 W/(m²K)
* **F value:** 0.78
* **Water resistance up to**: 900 Pa in closed position
* **Water resistance up to**: 150 Pa in open position
* **Leakage rate at 50 Pa**: < 15% (in closed position)
* **Burglar resistance**: class 2 (if window is WK2)
* **Sound damping Dn,e,w (C;Ctr):**
* In open position: 31(-1;-2) dB
* In closed position: 51 (-1;-3) dB

|  |  |
| --- | --- |
| **Properties:** | |
| Airflow Q at 1 Pa | 10.6 l/s/m |
| Airflow Q at 1 Pa | 38.1 m³/h/m |
| Airflow Q at 2 Pa | 17.2 l/s/m |
| Airflow Q at 2 Pa | 62.0 m³/h/m |
| Airflow Q at 10 Pa | 16.4 l/s/m |
| Airflow Q at 20 Pa | 19.2 l/s/m |
| Equivalent area | 13479 mm²/m |
| Self-regulating | yes |
| Surface area | 0.065 m²/m |